API 5L X56 Pipes, Tubulars and Hollow Section

Structural Seamless Tubes

Standard range of high yield structural tubes includes the following specifications:

API 5L X52 Modified

BS 7191 355EM, BS7191 355EMZ

EN 10210 S355 J2H (MOD)

API 5L X56, X60, X65, X70

BS 7191 450EM, BS7191 450EMZ

All Structural Seamless Tubes are supplied as follows:

Fully weldable

Yield range from 50Ksi - 100Ksi

Low temperature impact tested @ -20oC -40oC -50oC

All material fully certified to EN 10204 3.1b or 3.1c as required

Additional testing services (NAMAS Approved Test Houses)

Available in random and double random lengths between 6m-14m

Longer lengths and a full cutting service available on request

Supply Condition

Normalised

Hot Finished seamless pipe

Quenched and Tempered

As Rolled

S.A.W. Submerged Arc Welding Tubulars

We offer a complete range of welded tubulars custom fabricated to order. Welded tubulars are available in specifications and supply conditions as required including;

API 5LB

API 5L X52-X70

API 2H Grade 50

BS 7191 355D & DZ

BS 7191 355EM

BS 7191 355EMZ

BS 7191 450EM

BS 7191 450EMZ

ASTM A36

ASTM A572 Grade 50

ASTM A4130

Dillimax 690

S.H.S. Square Hollow Sections

Standard range of structural hollow sections include the following specifications:

EN10210 S275J2H (Former Grade 43D)

EN10210 S355J2H (Former Grade 50D)

Structural hollow sections are supplied as follows:

In standard & non standard sizes

Fully weldable

Low temperature impact tested @ -20oC

All material fully certified and Lloyds inspected

Additional NDT testing and third party inspection available on request

Lengths between 6m - 18m as standard

Longer lengths and a full cutting service available on request

Supply Condition

As rolled

If you have any other requirement for steel plate, please feel free to contact us.